Connected: An Internet Encyclopedia
RFC 1332

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments

Search: |  | Search Depth: |
Search Type: | String RegEx | Search Options: | NoCase WholeWord

Next: 1. Introduction

Network Working Group
Request for Comments: 1332
Obsoletes: RFC 1172

G. McGregor
Merit
May 1992

### The PPP Internet Protocol Control Protocol (IPCP)

#### Status of this Memo

This RFC specifies an IAB standards track protocol for the Internet community, and requests discussion and suggestions for improvements. Please refer to the current edition of the "IAB Official Protocol Standards" for the standardization state and status of this protocol. Distribution of this memo is unlimited.

#### Abstract

The Point-to-Point Protocol (PPP) [1] provides a standard method of encapsulating Network Layer protocol information over point-to-point links. PPP also defines an extensible Link Control Protocol, and proposes a family of Network Control Protocols (NCPs) for establishing and configuring different network-layer protocols.

This document defines the NCP for establishing and configuring the Internet Protocol [2] over PPP, and a method to negotiate and use Van Jacobson TCP/IP header compression [3] with PPP.

This RFC is a product of the Point-to-Point Protocol Working Group of the Internet Engineering Task Force (IETF).

#### Table of Contents

1. Introduction
2. A PPP Network Control Protocol (NCP) for IP

2.1. Sending IP Datagrams

3. IPCP Configuration Options

3.1. IP-Addresses
3.2. IP-Compression-Protocol
3.3. IP-Address

4. Van Jacobson TCP/IP header compression

4.1. Configuration Option Format

A. IPCP Recommended Options
Security Considerations
References
Acknowledgments
Chair's Address
Author's Address

Original text document

Next: 1. Introduction

Connected: An Internet Encyclopedia
RFC 1332