Connected: An Internet Encyclopedia
RFC 1157 - 3.2.6.3.6. egpNeighTable Object Type Names

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1157
Up: 3. The SNMP Architecture
Up: 3.2. Elements of the Architecture
Up: 3.2.6. Form and Meaning of References to Managed Objects
Up: 3.2.6.3. Identification of Object Instances
Prev: 3.2.6.3.5. tcpConnTable Object Type Names
Next: 4. Protocol Specification

### 3.2.6.3.6. egpNeighTable Object Type Names

The name of an EGP neighbor, x, is the OBJECT IDENTIFIER of the form a.b.c.d such that a.b.c.d is the value (in the familiar "dot" notation) of that instance of the egpNeighAddr object type associated with x.

For each object type, t, for which the defined name, n, has a prefix of egpNeighEntry, an instance, i, of t is named by an OBJECT IDENTIFIER of the form n.y, where y is the name of the EGP neighbor about which i represents information.

For example, suppose one wanted to find the neighbor state for the IP address of 89.1.1.42. Accordingly, egpNeighState.89.1.1.42 would identify the desired instance.

Next: 4. Protocol Specification

Connected: An Internet Encyclopedia
RFC 1157 - 3.2.6.3.6. egpNeighTable Object Type Names