Connected: An Internet Encyclopedia
RFC 1833 - 2.2 RPCBIND Operation

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1833
Up: 2. RPCBIND Program Protocol
Prev: 2.1 RPCBIND Protocol Specification (in RPC Language)
Next: 2.2.1 RPCBIND Version 3

### 2.2 RPCBIND Operation

RPCBIND is contacted by way of an assigned address specific to the transport being used. For TCP/IP and UDP/IP, for example, it is port number 111. Each transport has such an assigned, well-known address. The following is a description of each of the procedures supported by RPCBIND.

2.2.1 RPCBIND Version 3
2.2.2 RPCBIND, Version 4

Next: 2.2.1 RPCBIND Version 3

Connected: An Internet Encyclopedia
RFC 1833 - 2.2 RPCBIND Operation