Connected: An Internet Encyclopedia
RFC 1510 - A.16. KRB_PRIV generation

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1510
Up: A. Pseudo-code for protocol processing
Prev: A.15. KRB_SAFE and KRB_PRIV common checks
Next: A.17. KRB_PRIV verification

### A.16. KRB_PRIV generation

            collect user data in buffer;

            /* assemble packet: */
            packet.pvno := protocol version; /* 5 */
            packet.msg-type := message type; /* KRB_PRIV */

            packet.enc-part.etype := encryption type;

            body.user-data := buffer;
            if (using timestamp) then
                    get system_time;
                    body.timestamp, body.usec := system_time;
            endif
            if (using sequence numbers) then
                    body.seq-number := sequence number;
            endif
            body.s-address := sender host addresses;
            if (only one recipient) then
                    body.r-address := recipient host address;
            endif

            encode body into OCTET STRING;

            select encryption type;
            encrypt OCTET STRING into packet.enc-part.cipher;

Next: A.17. KRB_PRIV verification

Connected: An Internet Encyclopedia
RFC 1510 - A.16. KRB_PRIV generation