Connected: An Internet Encyclopedia
RFC 1907 - 2.6.2. Units of Conformance

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1907
Up: 2. Definitions
Up: 2.6. Conformance Information
Prev: 2.6.1. Compliance Statements
Next: 2.6.3. Obsolete Definitions

### 2.6.2. Units of Conformance

    -- units of conformance

    --  ::= { snmpMIBGroups 1 }           this OID is obsolete
    --  ::= { snmpMIBGroups 2 }           this OID is obsolete
    --  ::= { snmpMIBGroups 3 }           this OID is obsolete
    --  ::= { snmpMIBGroups 4 }           this OID is obsolete

    snmpGroup OBJECT-GROUP
        OBJECTS { snmpInPkts,
                  snmpInBadVersions,
                  snmpInASNParseErrs,
                  snmpSilentDrops,
                  snmpProxyDrops,
                  snmpEnableAuthenTraps }
        STATUS  current
        DESCRIPTION
                "A collection of objects providing basic instrumentation and
                control of an SNMPv2 entity."
        ::= { snmpMIBGroups 8 }

    snmpCommunityGroup OBJECT-GROUP
        OBJECTS { snmpInBadCommunityNames,
                  snmpInBadCommunityUses }
        STATUS  current
        DESCRIPTION
                "A collection of objects providing basic instrumentation of
                a SNMPv2 entity which supports community-based
                authentication."
        ::= { snmpMIBGroups 9 }

    snmpSetGroup OBJECT-GROUP
        OBJECTS { snmpSetSerialNo }
        STATUS  current
        DESCRIPTION
                "A collection of objects which allow several cooperating
                SNMPv2 entities, all acting in a manager role, to coordinate
                their use of the SNMPv2 set operation."
        ::= { snmpMIBGroups 5 }

    systemGroup OBJECT-GROUP
        OBJECTS { sysDescr, sysObjectID, sysUpTime,
                  sysContact, sysName, sysLocation,
                  sysServices,
                  sysORLastChange, sysORID,
                  sysORUpTime, sysORDescr }
        STATUS  current
        DESCRIPTION
                "The system group defines objects which are common to all
                managed systems."
        ::= { snmpMIBGroups 6 }

    snmpBasicNotificationsGroup NOTIFICATION-GROUP
        NOTIFICATIONS { coldStart, authenticationFailure }
        STATUS        current
        DESCRIPTION
                "The two notifications which an SNMPv2 entity is required to
                implement."
        ::= { snmpMIBGroups 7 }

Next: 2.6.3. Obsolete Definitions

Connected: An Internet Encyclopedia
RFC 1907 - 2.6.2. Units of Conformance