Connected: An Internet Encyclopedia
RFC 1421 - 4.5 Mail for Mailing Lists

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1421
Up: 4. Processing of Messages
Prev: 4.4 Encapsulation Mechanism
Next: 4.6 Summary of Encapsulated Header Fields

### 4.5 Mail for Mailing Lists

When mail is addressed to mailing lists, two different methods of processing can be applicable: the IK-per-list method and the IK-per- recipient method. Hybrid approaches are also possible, as in the case of IK-per-list protection of a message on its path from an originator to a PEM-equipped mailing list exploder, followed by IK- per-recipient protection from the exploder to individual list recipients.

If a message's originator is equipped to expand a destination mailing list into its individual constituents and elects to do so (IK-per- recipient), the message's DEK (and, in the symmetric key management case, MIC) will be encrypted under each per-recipient IK and all such encrypted representations will be incorporated into the transmitted message. Note that per-recipient encryption is required only for the relatively small DEK and MIC quantities carried in the "Key-Info:" field, not for the message text which is, in general, much larger. Although more IKs are involved in processing under the IK-per- recipient method, the pairwise IKs can be individually revoked and possession of one IK does not enable a successful masquerade of another user on the list.

If a message's originator addresses a message to a list name or alias, use of an IK associated with that name or alias as a entity (IK-per-list), rather than resolution of the name or alias to its constituent destinations, is implied. Such an IK must, therefore, be available to all list members. Unfortunately, it implies an undesirable level of exposure for the shared IK, and makes its revocation difficult. Moreover, use of the IK-per-list method allows any holder of the list's IK to masquerade as another originator to the list for authentication purposes.

Pure IK-per-list key management in the asymmetric case (with a common private key shared among multiple list members) is particularly disadvantageous in the asymmetric environment, as it fails to preserve the forwardable authentication and non-repudiation characteristics which are provided for other messages in this environment. Use of a hybrid approach with a PEM-capable exploder is therefore particularly recommended for protection of mailing list traffic when asymmetric key management is used; such an exploder would reduce (per discussion in Section 4.4 of this RFC) incoming ENCRYPTED messages to MIC-ONLY or MIC-CLEAR form before forwarding them (perhaps re-encrypted under individual, per-recipient keys) to list members.

Next: 4.6 Summary of Encapsulated Header Fields

Connected: An Internet Encyclopedia
RFC 1421 - 4.5 Mail for Mailing Lists