Connected: An Internet Encyclopedia
RFC 1812 - 2.1 Introduction

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1812
Up: 2. INTERNET ARCHITECTURE
Prev: 2. INTERNET ARCHITECTURE
Next: 2.2 Elements of the Architecture

### 2.1 Introduction

The Internet system consists of a number of interconnected packet networks supporting communication among host computers using the Internet protocols. These protocols include the Internet Protocol (IP), the Internet Control Message Protocol (ICMP), the Internet Group Management Protocol (IGMP), and a variety transport and application protocols that depend upon them. As was described in Section [1.2], the Internet Engineering Steering Group periodically releases an Official Protocols memo listing all the Internet protocols.

All Internet protocols use IP as the basic data transport mechanism. IP is a datagram, or connectionless, internetwork service and includes provision for addressing, type-of-service specification, fragmentation and reassembly, and security. ICMP and IGMP are considered integral parts of IP, although they are architecturally layered upon IP. ICMP provides error reporting, flow control, first-hop router redirection, and other maintenance and control functions. IGMP provides the mechanisms by which hosts and routers can join and leave IP multicast groups.

Reliable data delivery is provided in the Internet protocol suite by Transport Layer protocols such as the Transmission Control Protocol (TCP), which provides end-end retransmission, resequencing and connection control. Transport Layer connectionless service is provided by the User Datagram Protocol (UDP).

Next: 2.2 Elements of the Architecture

Connected: An Internet Encyclopedia
RFC 1812 - 2.1 Introduction