Connected: An Internet Encyclopedia
RFC 1771 - 6.4 NOTIFICATION message error handling.

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1771
Up: 6. BGP Error Handling.
Prev: 6.3 UPDATE message error handling.
Next: 6.5 Hold Timer Expired error handling.

### 6.4 NOTIFICATION message error handling.

If a peer sends a NOTIFICATION message, and there is an error in that message, there is unfortunately no means of reporting this error via a subsequent NOTIFICATION message. Any such error, such as an unrecognized Error Code or Error Subcode, should be noticed, logged locally, and brought to the attention of the administration of the peer. The means to do this, however, lies outside the scope of this document.

Next: 6.5 Hold Timer Expired error handling.

Connected: An Internet Encyclopedia
RFC 1771 - 6.4 NOTIFICATION message error handling.