Connected: An Internet Encyclopedia
RFC 1771 - 6.5 Hold Timer Expired error handling.

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1771
Up: 6. BGP Error Handling.
Prev: 6.4 NOTIFICATION message error handling.
Next: 6.6 Finite State Machine error handling.

### 6.5 Hold Timer Expired error handling.

If a system does not receive successive KEEPALIVE and/or UPDATE and/or NOTIFICATION messages within the period specified in the Hold Time field of the OPEN message, then the NOTIFICATION message with Hold Timer Expired Error Code must be sent and the BGP connection closed.

Next: 6.6 Finite State Machine error handling.

Connected: An Internet Encyclopedia
RFC 1771 - 6.5 Hold Timer Expired error handling.