Connected: An Internet Encyclopedia
RFC 1123 - 5.2.1 The SMTP Model: RFC-821 Section 2

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1123
Up: 5. ELECTRONIC MAIL -- SMTP and RFC-822
Up: 5.2 PROTOCOL WALK-THROUGH
Prev: 5.2 PROTOCOL WALK-THROUGH
Next: 5.2.2 Canonicalization: RFC-821 Section 3.1

### 5.2.1 The SMTP Model: RFC-821 Section 2

DISCUSSION:

  Mail is sent by a series of request/response transactions between a client, the "sender-SMTP," and a server, the "receiver-SMTP". These transactions pass (1) the message proper, which is composed of header and body, and (2) SMTP source and destination addresses, referred to as the "envelope".

  The SMTP programs are analogous to Message Transfer Agents (MTAs) of X.400. There will be another level of protocol software, closer to the end user, that is responsible for composing and analyzing RFC-822 message headers; this component is known as the "User Agent" in X.400, and we use that term in this document. There is a clear logical distinction between the User Agent and the SMTP implementation, since they operate on different levels of protocol. Note, however, that this distinction is may not be exactly reflected the structure of typical implementations of Internet mail. Often there is a program known as the "mailer" that implements SMTP and also some of the User Agent functions; the rest of the User Agent functions are included in a user interface used for entering and reading mail.

  The SMTP envelope is constructed at the originating site, typically by the User Agent when the message is first queued for the Sender-SMTP program. The envelope addresses may be derived from information in the message header, supplied by the user interface (e.g., to implement a bcc: request), or derived from local configuration information (e.g., expansion of a mailing list). The SMTP envelope cannot in general be re-derived from the header at a later stage in message delivery, so the envelope is transmitted separately from the message itself using the MAIL and RCPT commands of SMTP.

  The text of RFC-821 suggests that mail is to be delivered to an individual user at a host. With the advent of the domain system and of mail routing using mail-exchange (MX) resource records, implementors should now think of delivering mail to a user at a domain, which may or may not be a particular host. This DOES NOT change the fact that SMTP is a host-to-host mail exchange protocol.

Next: 5.2.2 Canonicalization: RFC-821 Section 3.1

Connected: An Internet Encyclopedia
RFC 1123 - 5.2.1 The SMTP Model: RFC-821 Section 2