Connected: An Internet Encyclopedia
RFC 1700 - service-names

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1700

Search: |  | Search Depth: |
Search Type: | String RegEx | Search Options: | NoCase WholeWord

    PROTOCOL AND SERVICE NAMES

    These are the Official Protocol Names as they appear in the Domain
    Name System WKS records and the NIC Host Table.  Their use is
    described in [RFC952].

    A protocol or service may be up to 40 characters taken from the set of
    uppercase letters, digits, and the punctuation character hyphen.  It
    must start with a letter, and end with a letter or digit.

    ARGUS               - ARGUS Protocol
    ARP                 - Address Resolution Protocol
    AUTH                - Authentication Service
    BBN-RCC-MON         - BBN RCC Monitoring
    BL-IDM              - Britton Lee Intelligent Database Machine
    BOOTP               - Bootstrap Protocol
    BOOTPC              - Bootstrap Protocol Client
    BOOTPS              - Bootstrap Protocol Server
    BR-SAT-MON          - Backroom SATNET Monitoring
    CFTP                - CFTP
    CHAOS               - CHAOS Protocol
    CHARGEN             - Character Generator Protocol
    CISCO-FNA           - CISCO FNATIVE
    CISCO-TNA           - CISCO TNATIVE
    CISCO-SYS           - CISCO SYSMAINT
    CLOCK               - DCNET Time Server Protocol
    CMOT                - Common Mgmnt Info Ser and Prot over TCP/IP
    COOKIE-JAR          - Authentication Scheme
    CSNET-NS            - CSNET Mailbox Nameserver Protocol
    DAYTIME             - Daytime Protocol
    DCN-MEAS            - DCN Measurement Subsystems Protocol
    DCP                 - Device Control Protocol
    DGP                 - Dissimilar Gateway Protocol
    DISCARD             - Discard Protocol
    DMF-MAIL            - Digest Message Format for Mail
    DOMAIN              - Domain Name System
    ECHO                - Echo Protocol
    EGP                 - Exterior Gateway Protocol
    EHF-MAIL            - Encoding Header Field for Mail
    EMCON               - Emission Control Protocol
    EMFIS-CNTL          - EMFIS Control Service
    EMFIS-DATA          - EMFIS Data Service
    FCONFIG             - Fujitsu Config Protocol
    FINGER              - Finger Protocol
    FTP                 - File Transfer Protocol
    FTP-DATA            - File Transfer Protocol Data
    GGP                 - Gateway Gateway Protocol
    GRAPHICS            - Graphics Protocol
    HMP                 - Host Monitoring Protocol
    HOST2-NS            - Host2 Name Server
    HOSTNAME            - Hostname Protocol
    ICMP                - Internet Control Message Protocol
    IGMP                - Internet Group Management Protocol
    IGP                 - Interior Gateway Protocol
    IMAP2               - Interim Mail Access Protocol version 2
    INGRES-NET          - INGRES-NET Service
    IP                  - Internet Protocol
    IPCU                - Internet Packet Core Utility
    IPPC                - Internet Pluribus Packet Core
    IP-ARC              - Internet Protocol on ARCNET
    IP-ARPA             - Internet Protocol on ARPANET
    IP-CMPRS            - Compressing TCP/IP Headers
    IP-DC               - Internet Protocol on DC Networks
    IP-DVMRP            - Distance Vector Multicast Routing Protocol
    IP-E                - Internet Protocol on Ethernet Networks
    IP-EE               - Internet Protocol on Exp. Ethernet Nets
    IP-FDDI             - Transmission of IP over FDDI
    IP-HC               - Internet Protocol on Hyperchannnel
    IP-IEEE             - Internet Protocol on IEEE 802
    IP-IPX              - Transmission of 802.2 over IPX Networks
    IP-MTU              - IP MTU Discovery Options
    IP-NETBIOS          - Internet Protocol over NetBIOS Networks
    IP-SLIP             - Transmission of IP over Serial Lines
    IP-WB               - Internet Protocol on Wideband Network
    IP-X25              - Internet Protocol on X.25 Networks
    IRTP                - Internet Reliable Transaction Protocol
    ISI-GL              - ISI Graphics Language Protocol
    ISO-TP4             - ISO Transport Protocol Class 4
    ISO-TSAP            - ISO TSAP
    LA-MAINT            - IMP Logical Address Maintenance
    LARP                - Locus Address Resoultion Protocol
    LDP                 - Loader Debugger Protocol
    LEAF-1              - Leaf-1 Protocol
    LEAF-2              - Leaf-2 Protocol
    LINK                - Link Protocol
    LOC-SRV             - Location Service
    LOGIN               - Login Host Protocol
    MAIL                - Format of Electronic Mail Messages
    MERIT-INP           - MERIT Internodal Protocol
    METAGRAM            - Metagram Relay
    MIB                 - Management Information Base
    MIT-ML-DEV          - MIT ML Device
    MFE-NSP             - MFE Network Services Protocol
    MIT-SUBNET          - MIT Subnet Support
    MIT-DOV             - MIT Dover Spooler
    MPM                 - Internet Message Protocol (Multimedia Mail)
    MPM-FLAGS           - MPM Flags Protocol
    MPM-SND             - MPM Send Protocol
    MSG-AUTH            - MSG Authentication Protocol
    MSG-ICP             - MSG ICP Protocol
    MUX                 - Multiplexing Protocol
    NAMESERVER          - Host Name Server
    NETBIOS-DGM         - NETBIOS Datagram Service
    NETBIOS-NS          - NETBIOS Name Service
    NETBIOS-SSN         - NETBIOS Session Service
    NETBLT              - Bulk Data Transfer Protocol
    NETED               - Network Standard Text Editor
    NETRJS              - Remote Job Service
    NI-FTP              - NI File Transfer Protocol
    NI-MAIL             - NI Mail Protocol
    NICNAME             - Who Is Protocol
    NFILE               - A File Access Protocol
    NNTP                - Network News Transfer Protocol
    NSW-FE              - NSW User System Front End
    NTP                 - Network Time Protocol
    NVP-II              - Network Voice Protocol
    OSPF                - Open Shortest Path First Interior GW Protocol
    PCMAIL              - Pcmail Transport Protocol
    POP2                - Post Office Protocol - Version 2
    POP3                - Post Office Protocol - Version 3
    PPP                 - Point-to-Point Protocol
    PRM                 - Packet Radio Measurement
    PUP                 - PUP Protocol
    PWDGEN              - Password Generator Protocol
    QUOTE               - Quote of the Day Protocol
    RARP                - A Reverse Address Resolution Protocol
    RATP                - Reliable Asynchronous Transfer Protocol
    RE-MAIL-CK          - Remote Mail Checking Protocol
    RDP                 - Reliable Data Protocol
    RIP                 - Routing Information Protocol
    RJE                 - Remote Job Entry
    RLP                 - Resource Location Protocol
    RTELNET             - Remote Telnet Service
    RVD                 - Remote Virtual Disk Protocol
    SAT-EXPAK           - Satnet and Backroom EXPAK
    SAT-MON             - SATNET Monitoring
    SEP                 - Sequential Exchange Protocol
    SFTP                - Simple File Transfer Protocol
    SGMP                - Simple Gateway Monitoring Protocol
    SNMP                - Simple Network Management Protocol
    SMI                 - Structure of Management Information
    SMTP                - Simple Mail Transfer Protocol
    SQLSRV              - SQL Service
    ST                  - Stream Protocol
    STATSRV             - Statistics Service
    SU-MIT-TG           - SU/MIT Telnet Gateway Protocol
    SUN-RPC             - SUN Remote Procedure Call
    SUPDUP              - SUPDUP Protocol
    SUR-MEAS            - Survey Measurement
    SWIFT-RVF           - Remote Virtual File Protocol
    TACACS-DS           - TACACS-Database Service
    TACNEWS             - TAC News
    TCP                 - Transmission Control Protocol
    TCP-ACO             - TCP Alternate Checksum Option
    TELNET              - Telnet Protocol
    TFTP                - Trivial File Transfer Protocol
    THINWIRE            - Thinwire Protocol
    TIME                - Time Server Protocol
    TP-TCP              - ISO Transport Service on top of the TCP
    TRUNK-1             - Trunk-1 Protocol
    TRUNK-2             - Trunk-2 Protocol
    UCL                 - University College London Protocol
    UDP                 - User Datagram Protocol
    NNTP                - Network News Transfer Protocol
    USERS               - Active Users Protocol
    UUCP-PATH           - UUCP Path Service
    VIA-FTP             - VIA Systems-File Transfer Protocol
    VISA                - VISA Protocol
    VMTP                - Versatile Message Transaction Protocol
    WB-EXPAK            - Wideband EXPAK
    WB-MON              - Wideband Monitoring
    XNET                - Cross Net Debugger
    XNS-IDP             - Xerox NS IDP

    REFERENCES

    [RFC952] Harrenstien, K., Stahl, M., and E. Feinler, "DoD Internet
             Host Table Specification", RFC 952, SRI, October 1985.

    []

Connected: An Internet Encyclopedia
RFC 1700 - service-names