Connected: An Internet Encyclopedia
RFC 1906 - 1. Introduction

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1906
Next: 1.1. A Note on Terminology

### 1. Introduction

A management system contains: several (potentially many) nodes, each with a processing entity, termed an agent, which has access to management instrumentation; at least one management station; and, a management protocol, used to convey management information between the agents and management stations. Operations of the protocol are carried out under an administrative framework which defines authentication, authorization, access control, and privacy policies.

Management stations execute management applications which monitor and control managed elements. Managed elements are devices such as hosts, routers, terminal servers, etc., which are monitored and controlled via access to their management information.

The management protocol, version 2 of the Simple Network Management Protocol [1], may be used over a variety of protocol suites. It is the purpose of this document to define how the SNMPv2 maps onto an initial set of transport domains. Other mappings may be defined in the future.

Although several mappings are defined, the mapping onto UDP is the preferred mapping. As such, to provide for the greatest level of interoperability, systems which choose to deploy other mappings should also provide for proxy service to the UDP mapping.

1.1. A Note on Terminology

Next: 1.1. A Note on Terminology

Connected: An Internet Encyclopedia
RFC 1906 - 1. Introduction