Connected: An Internet Encyclopedia
RFC 1902 - 8.6. Usage Example

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1902
Up: 8. Mapping of the NOTIFICATION-TYPE macro
Prev: 8.5. Mapping of the NOTIFICATION-TYPE value
Next: 9. Refined Syntax

### 8.6. Usage Example

Consider how a linkUp trap might be described:

    linkUp NOTIFICATION-TYPE
        OBJECTS { ifIndex }
        STATUS  current
        DESCRIPTION
                "A linkUp trap signifies that the SNMPv2 entity, acting in
                an agent role, recognizes that one of the communication
                links represented in its configuration has come up."
        ::= { snmpTraps 4 }

According to this invocation, the trap authoritatively identified as

         { snmpTraps 4 }

is used to report a link coming up.

Next: 9. Refined Syntax

Connected: An Internet Encyclopedia
RFC 1902 - 8.6. Usage Example