Connected: An Internet Encyclopedia
RFC 793 - 2.3. The Host Environment

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 793
Up: 2. PHILOSOPHY
Prev: 2.2. Model of Operation
Next: 2.4. Interfaces

### 2.3. The Host Environment

The TCP is assumed to be a module in an operating system. The users access the TCP much like they would access the file system. The TCP may call on other operating system functions, for example, to manage data structures. The actual interface to the network is assumed to be controlled by a device driver module. The TCP does not call on the network device driver directly, but rather calls on the internet datagram protocol module which may in turn call on the device driver.

The mechanisms of TCP do not preclude implementation of the TCP in a front-end processor. However, in such an implementation, a host-to-front-end protocol must provide the functionality to support the type of TCP-user interface described in this document.

Next: 2.4. Interfaces

Connected: An Internet Encyclopedia
RFC 793 - 2.3. The Host Environment