;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
;;
;;  NetMos Technology, inc.
;;
;;  FILE : NmMfEnum.inf
;;  This file works in conjunction with nmmfenum.vxd.
;;  OS SUPPORTED : WIN98 ONLY.
;;
;;  See NmMfEnum.Hw.AddReg section to enable/disable
;;  re-mapping serial/parallel port iobase to legacy ports
;;  like 3F8, 2F8, etc.
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;

[Version]
LayoutFile = layout.inf
Signature  = $CHICAGO$
Class      = NetMosMultiFunction
Provider   = %ProviderName%
DriverVer  = 02/16/2002

[DestinationDirs]
DefaultDestDir  = 11    ;LDID_SYS
Inf.Copy = 17       	;DIRID_INF

[SourceDiskFiles]
; 1 = Disk Number
NmMfEnum.inf=1
NmEnum.inf=1
NmSNull.inf=1
NmPorts.inf=1
NmEnum.vxd=1
NmMfEnum.vxd=1
NmUninst.exe=1

[SourceDisksNames]
1=%DiskName%,,

;------------------------
; Install CLass 
;------------------------
[ClassInstall]
CopyFiles=Inf.Copy,Uninstall.Copy
AddReg=Class.AddReg

[Class.AddReg]
HKR,,Icon,,-23

[Manufacturer]
%MfgName%=NetMosCards

;------------------------
; Install Drivers
;------------------------
[NetMosCards]
%Nm9805Name%=NmMfEnum,PCI\VEN_9710&DEV_9805
%Nm9815Name%=NmMfEnum,PCI\VEN_9710&DEV_9815
%Nm9820Name%=NmMfEnum,PCI\VEN_9710&DEV_9820
%Nm9825Name%=NmMfEnum,PCI\VEN_9710&DEV_9825
%Nm9835Name%=NmMfEnum,PCI\VEN_9710&DEV_9835
%Nm9845Name%=NmMfEnum,PCI\VEN_9710&DEV_9845
%Nm9855Name%=NmMfEnum,PCI\VEN_9710&DEV_9855

[NmEnum]
CopyFiles=Inf.Copy,NmEnum.Copy,Uninstall.Copy
AddReg=NmEnum.AddReg,Uninstall.AddReg

[NmEnum.AddReg]
HKR,,DevLoader,0,NMENUM.vxd

[NmMfEnum]
CopyFiles=Inf.Copy,NmMfEnum.Copy,Uninstall.Copy
AddReg=NmMfEnum.AddReg,Uninstall.AddReg
UpdateAutoBat=NmDosIn.AutoBat

[NmMfEnum.Hw]
AddReg=NmMfEnum.Hw.AddReg

[NmMfEnum.AddReg]
HKR,,DevLoader,0,NMMFENUM.vxd

;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
; NmMfEnum.Hw.AddReg Section
;
; Remap To Legacy I/O Ports
;
; The following line will enable Remap of serial/parallel ports
; HKR,,RemapToLegacyPort,1,1
; The following line will disable Remap of serial/parallel ports
; HKLM,Enum\NMMFENUM\PCI9710_COM,RemapToLegacyPort,1,1
;
; DEFAULT Action is to enable remapping. If the line 
; RemapToLegacyPort line is not present here, then driver
; will enable the remapping of LPT/COM ports. 
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
[NmMfEnum.Hw.AddReg]
HKR,,RemapToLegacyPort,1,1

[Uninstall.AddReg]
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Uninstall\%MfgName%,DisplayName,0,%UninstallName%
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Uninstall\%MfgName%,UninstallString,0,NmUninst.exe

[Inf.Copy]
NmEnum.inf
NmMfEnum.inf
NmSNull.inf
NmPorts.inf

[NmEnum.Copy]
NMENUM.vxd

[NmMfEnum.Copy]
NMMFENUM.vxd

[Uninstall.Copy]
NmUninst.exe

[NmDosIn.AutoBat]
PrefixPath=11
CmdDelete=NmDosIn
;CmdAdd=NmDosIn,"-a -r -s"

[Strings]
ProviderName="NetMos Technology"
MfgName="NetMos Technology"
DiskName="NetMos Multi I/O Driver Disk"
UninstallName="NetMos Multi-IO Controller"
ComPortName="NetMos PCI Serial Port"
LptPortName="NetMos PCI Parallel Port"
EcpPortName="NetMos PCI SPP/BPP/ECP/EPP Port"
NullPortName="NetMos Bridge"
Nm9705Name="NetMos PCI 9705 Parallel Port"
Nm9735Name="NetMos PCI 9735 Multi-I/O Controller"
Nm9745Name="NetMos PCI 9745 Multi-I/O Controller"
NmS9705Name="NetMos PCI 9705 Parallel Port"
NmS9735Name="NetMos PCI 9735 Serial Port"
NmS9745Name="NetMos PCI 9745 Serial Port"
Nm9805Name="NetMos PCI 9805 Parallel Port"
Nm9815Name="NetMos PCI 9815 Multi-I/O Controller"
Nm9820Name="NetMos PCI 9820 Serial Port"
Nm9825Name="NetMos PCI 9825 Serial Port"
Nm9835Name="NetMos PCI 9835 Multi-I/O Controller"
Nm9845Name="NetMos PCI 9845 Multi-I/O Controller"
Nm9855Name="NetMos PCI 9855 Multi-I/O Controller"

; END OF FILE

