Canon Advanced Printing Technology for Canon LBP-800   R1.01
******************************************************************

Thank you for purchasing the Canon Laser Beam Printer LBP-800,
with enhanced performance and ease-of-use from the Canon Advanced 
Printing Technology.  We hope that you'll appreciate its 
exceptional print quality, flexible paper handling, fast printing 
speed, and trouble-free operation.

Your best source of information on this product is the Canon 
LBP-800 On-Line Help and the Canon LBP-800 On-Line Manuals.

This README file has been created to address some very important 
or specific issues that may be encountered during the use of this 
product.

==================================================================

Contents:

1. Scaling
2. Overlay
3. Halftone
4. Toner Saver
5. Sharing a parallel port with another device
6. ECP settings: Windows 9x
7. Printing On-Line Help: Windows NT
8. Uninstalling network printer that other user connected: Windows NT
9. Restriction on Windows NT network printer
10. Restarting Windows with a remaining print job: Windows NT
==================================================================

1. Scaling

Some applications may not print correctly when scaling is set at 
other than 100% by LBP-800 Printer Setup or Properties. In this 
case, please set its scaling at 100%. If the application has own 
its scaling function, please set scaling from the application.

==================================================================

2. Overlay

Depending on its application, the printout using overlay form may 
be different from what you expect to be printed. For example, the 
contents of overlay form beyond the printing area may not be 
printed unless changing its printing area (or margin) setting. 
Please try to print it setting its margin as wide as to fit all 
contents of overlay form in the printable area.

==================================================================

3. Halftone

The Halftone settings are valid when printing colored bitmap, 
area filling, and colored text. However the Smooth setting is 
only valid when printing colored bitmap.

==================================================================

4. Toner Saver

Using Toner Saver mode, the objects filled with some graphic 
patterns may not be printed as shown on the display.

==================================================================

5. Sharing a parallel port with another device

LBP-800 is capable of sharing a parallel port with another device 
such as a scanner which conforms to the contention management 
described in DDK (Device Driver Development Kit). When both 
devices are, however, used simultaneously, this may cause a 
problem with an operation.

==================================================================

6. ECP settings: Windows 9x

Depending on the PC in use, the printout may not come out 
properly if "ECP with DMA" is used. In such a case, please select 
"ECP without DMA" or "Standard" in the Port Setting dialog box 
using the Printer Status Window. If the problem is not resolved 
by this, you may be able to solve this by changing its BIOS setup 
(i.e. parallel port mode or parallel port address).

==================================================================

7. Printing On-Line Help: Windows NT

If you want to print the contents of the On-Line Help, start up 
the [Canon LBP-800 Help] from the Canon CAPT Tools group.

==================================================================

8. Uninstalling network printer that other user connected: Windows NT

When you execute the [Canon LBP-800 Uninstallation] on the PC 
that other user have already connected to the Canon LBP-800 
network printer servers, information of the Canon LBP-800 network 
printer that other user connected will not be removed. In this 
case, other user should remove his Canon LBP-800 printer icon 
before you execute uninstallation.

==================================================================

9. Restriction on Windows NT network printer

When a network printer is installed on Windows NT, even though 
you change its connection destination to a local port, the 
printer cannot be used as a local printer. If you need to 
establish a local printer, you must install a printer driver, 
selecting a local port.

==================================================================

10. Restarting Windows with a remaining print job: Windows NT

If you need to restart Windows NT with a remaining LBP-800 print 
job, first double-click the LBP-800 in the Printers folder and 
pause the print job. 
Then restart Windows NT.

==================================================================

<END OF README.TXT>
