AdeptXbbs

*****************************************************************************

DisClaimer:

1> This software is now *SHARE*ware and as such I assume no responsibility
   for ANYthing that it may or may not do, by running this software
   you agree to free me from any kind of liabilty whatsoever resulting
   from damages or losses incurred by running this software. I have tried
   to make it as bugfree and foolproof as possible, but no program is perfect.

   I cannot accept any responsibility for any damages. I will try to do my
   best to fix reproducible bugs as they are reported, but I work on this hobby
   in my spare time so don't get mad if the bug does not get fixed right away.


2> Registration is only $20.00 in U.S. funds, policy and licence
   is simple, u use it, u should register it, one copy paid for
   means u run it on one machine at a time (that machine can run
   as many instances (see below) of that copy as u think the hardware
   and os will stand) if you're networking two or more machines,
   I expect two or more registrations. There are no cripples,
   or nags or reminders or time bombs in my software, I simply
   appeal to your conscience to do the right thing and send in that reg
   fee.

3> Registration puts you in my DataBase for free upgrades
   and bugfixe releases, free till such time as I think
   a release is a major upgrade and warrants an upgrade
   fee (prolly nominal, but what the hell). Support will be
   done on a best effort basis, I have an e-mail address
   which I'll post further on in this document. I also drop
   into #adept on irc server irc.isonline.com from time to time
   and if u catch me there I'll try to help you with anything
   I can, there are other adept sysops there as well.


3> That said, updates can be had at hobbes.nmsu.edu.
   Look for adeptfull.zip and adeptupgrade.zip. These two
   archives will have the latest code in them.

4> email me at mariod@ican.net
        Send Reg Fees to
        Mario D'Ulisse
        4 Paladin Ave.
        Sault Ste. Marie,ON
        Canada
        P6B-3P6

        Send $20.00 U.S. per copy in postal money order
        form, personal check or any other easily cashed
        form. Please don't send Cash in the mail.



******************************************************************************
4.1w
1> This build should be a drop in replacemnt for adept111 and down
   by following these simple steps,
   1> Delete all *_Configuration files in \adept
   2> Delete All *.Bin files in \adept\menus
   3> Fire it up in /setup mode, configure to your liking,
      shut it down, and bring it online normally.
2> Note: the users file should be safe but back it up just in case

4.1u
1> Adept now supports 6144 nodes PER COPY *BUT* you can run as many copies
   as u have machine or network to support, they will all quite happily share
   all config files cept for the linex configuration and log files. These are specific
   to the Case (instance) of adept running, but msg/files/user/bbs/menus/text
   etc configs are the same for all copies, giving u virtually unlimited nodes
   outta the box. To start a second copy of adept just type Adept /Nodes x /StartAt 2
   where x is number of nodes for this copy up to 6144 and 2 is instance 2 of adept.
   just replace the 2 with a 3 for a third instance and so forth.
   Note that when running multiple instances of adept there is only 1 outbound manager
   it lives on the first instance only. However mailer nodes are active on all
   instances unless u check the no mailer option for a particular node that is.
   Note: That OS/2 only supports 4k threads and each node of adept is a thread,
   so......<g>



4.1t
1> After much fuqing around with watcom v11.0a and repeated calls to tech support
   we have come to the conclusion that it is broken as far as compiling a large
   complex project like adept, they have kindly given me a copy of 10.6a which
   seems to be compiling/linking adept just dandy.
   Recompiled all code that i have access to with the new compiler.
2> More miscellaneous cleanup and general speed improvements, started 384
   nodes here on my machine with 48 megs o ram and a 48 meg swap file before
   I ran out of threads, can prolly start 512 on my configuration, anyway
   this build supports 2048 nodes outta the box, would love to see the machine
   with the memory to run this beast, note startup and shutdown are kind slow
   since it takes time to close/open all the various logfiles for each node,
   shutdown can be hurried up by clicking close in the upper left pulldown stead of
   the usual shutdown on/off hook selection.
3> Line configs and events files are no longer saved on a shutdown *UNLESS*
   you started Adept with the /SETUP option, same for colors and fonts and window
   positions.
4> Added a new command line switch /BEEPS will enable an audible tone on a
   successfull connect to adept on any online node ala SIO's telnet connection
   tone (rememeber that?). If u prefer quiet operation, this switch is not for you.
5> Fixed a memory alloc problem in ansi display routines, was a possible trap
   condition on large files.
6> Increased the total process wide stack space available, this should cure
   some of the spurious traps executing large complex AdeptRexx routines,
   specially those which call adeptmenutype or adeptmenu functions, as the code
   recurses a lot during this execution.
7> Reworked the line configs storage allocation yet again.
8> This build requires u delete all *_CONFIGURATION files in \adept dir
   and all *.bin files in \adept\menus dir and do a /setup to recreate
   them.
9> Set the default line creation configs to telnet ports as most people
   will likely only have a handfull of real modems and its easier to
   edit the few nodes for real modems than 50 telnet nodes, the telnet
   nodes come setup ready to use, just enable the telnet server in internet
   options under config pulldown to start using them.

