
                   comp.os.os2.setup                (Usenet)

                 Saturday, 09-Oct-1999 to Friday, 15-Oct-1999

+----------------------------------------------------------------------------+

From: davisfnospam@union.edu                            09-Oct-99 17:28:24
  To: All                                               09-Oct-99 19:56:26
Subj: Re: Installing FIX-pack_try QF11

From: davisfnospam@union.edu

In <37FAC186.60B0A46F@my-deja.com>, on 10/06/99 
   at 03:31 AM, luistino <luistino@my-deja.com> said:


>I cannot remember where I downloaded from, probaly hoobes, look for
>Qf11.zip

There is a small bug in this program which I don't know has been fixed. In
the file called install.fil, your archive directory won't be correctly
input; you have to modify this file by hand. I believe the newest version
also handles fixpak zip files. 

I got this info from some helpful sources. I used QF last week to install
FP11 on my laptop and I'm going to use it to install FP12 soon on my
desktop.

F.

-----------------------------------------------------------
      Felmon John Davis		
     davisf@union.edu	|  davisf@capital.net     
     Union College /  Schenectady, NY
     - insert standard doxastic disclaimers -
     OS/2 - ma kauft koi katz em sack 
-----------------------------------------------------------

--- WtrGate+ v0.93.p7 sn 165
 * Origin: Usenet: Logical Net (1:109/42)

+----------------------------------------------------------------------------+

From: dwparsons@t-online.de                             10-Oct-99 13:15:15
  To: All                                               10-Oct-99 10:22:27
Subj: Re: Installing FIX-pack

From: dwparsons@t-online.de (Dave Parsons)

On Tue, 5 Oct 1999 09:37:58, "Mackan" <Mackan@SpamMeNot.se> wrote:

> Hello there
> 
> I was trying to install the fixpack (fixpack 11 for os/2 warp 4.) , not
> using diskettes or the web.

 < snip >
 
> Any suggestions how to succseed in applying a fixpack is very helpful.
> I have applyed the FIXpack 7 on this computer, but that was a year ago, and
> I did use disketts then, but I hade disketts,
> so I wanna figure this out, so I don't have to use the disks.
> Why havn't IBM figured out an easy way to upgrade OS/2.
 
The easiest & quickest way that I have found is to download the *.zip
files from the RSU site and then follow the instructions given in an
article by Walter Metcalf.

http://os2.miningco.com/library/weekly/aa111898.htm

BTW, don't bother with FP11, go for FP12

-- 
Dave

--- WtrGate+ v0.93.p7 sn 165
 * Origin: Usenet: CDL (1:109/42)

+----------------------------------------------------------------------------+

From: jmcnamar@optonline.net                            10-Oct-99 16:21:23
  To: All                                               10-Oct-99 16:28:10
Subj: cable modem configuring

From: John McNamara <jmcnamar@optonline.net>

I have a Optimum Online Cable modem hooked up into a ne2000 ethernet
card.  Can anyone please point me in the direction on how to configure
this so as I can access the Internet thru my Cable Modem.  The NIC is
set for IRQ 10 and IO 0x300.  I installed tcp/ip on the Warp 4 box and
tried to configure it t  no avail.  Any help or shoves in the right
direction would be appreciated.  Alose are there any FAQs out there on
this subject re: Configureing Network Adapters   or  Configuring Cable
Modems  ?

TIA


John McNamara

jmcnamar@optonline.net

--- WtrGate+ v0.93.p7 sn 165
 * Origin: Usenet: Optimum Online (1:109/42)

+----------------------------------------------------------------------------+

From: james.arnold@!!!usa.net                           10-Oct-99 17:08:08
  To: All                                               10-Oct-99 16:28:10
Subj: Re: cable modem configuring

From: james.arnold@!!!usa.net

In <3800BC88.B19A4B74@optonline.net>, John McNamara <jmcnamar@optonline.net>
writes:
>I have a Optimum Online Cable modem hooked up into a ne2000 ethernet
>card.  Can anyone please point me in the direction on how to configure
>this so as I can access the Internet thru my Cable Modem.  The NIC is
>set for IRQ 10 and IO 0x300.  I installed tcp/ip on the Warp 4 box and
>tried to configure it t  no avail.  Any help or shoves in the right

	Note that there is nothing inherently different about a cable modem and
a router, which in essense it is. What you have to do is first make sure that
you NIC is configured properly along with Warp's software.

	Did you choose the Networking install? Does the NIC driver load
properly at boot?

	The first thing I would do is check your networking software setup.
Run MPTS to check for basic networking commponents. remove all transports
except for TCP/IP if there are others. It is much easier to get one working
properly and then install others that are needed. Once you are sure that the
basic networking components are installed and configured properly then go
to the TCP/IP configuration notebook and configure TCP/IP. Make sure that
you include the loopback adapter. It will allow you to check your TCP/IP
configuration locally. You should be able to do a successful "ping localhost".

	Once you get this working then set up the parameters that your ISP
has given you for DNS, whether or not to use DHCP or a static IP address
your domain name, possibly a host name, a gateway/router address.

>direction would be appreciated.  Alose are there any FAQs out there on
>this subject re: Configureing Network Adapters   or  Configuring Cable
>Modems  ?

	There are lots of pages with info about cable modems, some that come
to mind:

	for RoadRunner info - http://Larkin.NuclearWinter.com/rros2/
	Connecting a home LAN to the Internet :
		http://nateliskov.ne.mediaone.net/network/homenet.htm

	General information links: Warp on the Net - http://www.nfwa.com/os2/

	Once you get the above configuration done and have perused the links,
if you still have problems get back to use with as much information as
possible.
I am sure we will be able to point you in the right direction.

	Jim


===========================================================================
remove !!! for e-mail
James Arnold                                email:    james.arnold@usa.net
                                              ICQ:    9719182

        Member Toronto OS/2 User Group

Brought to you by the letters O S the number 2 and NR/2
===========================================================================

--- WtrGate+ v0.93.p7 sn 165
 * Origin: Usenet: Sympatico (1:109/42)

+----------------------------------------------------------------------------+

From: Spammers@Bite.Me                                  10-Oct-99 18:38:25
  To: All                                               10-Oct-99 19:57:00
Subj: Re: cable modem configuring

From: "Jaime A. Cruz, Jr." <Spammers@Bite.Me>

-----BEGIN PGP SIGNED MESSAGE-----
Hash: SHA1

From: "Jaime A. Cruz, Jr." <Spammers@Bite.Me>
Message-ID: <wnvzrpbcgbayvararg.fjeh4p1.pminews@news.optonline.net>
References:  <3800BC88.B19A4B74@optonline.net>
Date: Sun, 10 Oct 1999 14:38:49 -0400 (EDT)
Reply-To: "Jaime A. Cruz, Jr." <Spammers@Bite.Me>
X-Newsreader: PMINews 2.00.1205 For OS/2
Organization: Nassau Wings Motorcycle Club
MIME-Version: 1.0
Content-Type: text/plain; charset="us-ascii"
Content-Transfer-Encoding: 7bit
Subject: Re: cable modem configuring

I'm running a similar setup.  Make sure you have the latest updates to the
TCP/IP stack and MPTS, then configure the  LAN card for DHCP.  That's all you
should have to do!

On Sun, 10 Oct 1999 16:21:47 GMT, John McNamara wrote:

>I have a Optimum Online Cable modem hooked up into a ne2000 ethernet
>card.  Can anyone please point me in the direction on how to configure
>this so as I can access the Internet thru my Cable Modem.  The NIC is
>set for IRQ 10 and IO 0x300.  I installed tcp/ip on the Warp 4 box and
>tried to configure it t  no avail.  Any help or shoves in the right
>direction would be appreciated.  Alose are there any FAQs out there on
>this subject re: Configureing Network Adapters   or  Configuring Cable
>Modems  ?
>
>TIA
>
>
>John McNamara
>
>jmcnamar@optonline.net
>

Jaime A. Cruz, Jr.

o&o_o&o_o&o_o&o_o&o_o&o_o&o_o&o_o&o_o&o_o&o_o&o_o&o
o                                                 o
o  Visit the Nassau Wings Motorcycle Club at:     o
o  http://www.nassauwings.org/                    o
o  A Charter Member of the Motorcycle Web Ring!   o
o                                                 o
o&o_o&o_o&o_o&o_o&o_o&o_o&o_o&o_o&o_o&o_o&o_o&o_o&o



-----BEGIN PGP SIGNATURE-----
Version: PGPfreeware 5.0 OS/2 for non-commercial use
Comment: PGP 5.0 for OS/2
Charset: cp850

wj8DBQE4AM8pgvzYfxgMc34RAtvCAJ9OV7z/VoWJ0EovvV5J0ApWaPC6NwCgxNBR
qWDKJ3JWy8NaBMzv+jensz4=
=dBvV
-----END PGP SIGNATURE-----

--- WtrGate+ v0.93.p7 sn 165
 * Origin: Usenet: Nassau Wings Motorcycle Club (1:109/42)

+----------------------------------------------------------------------------+

From: ysme@sympatico.ca                                 11-Oct-99 22:16:28
  To: All                                               11-Oct-99 21:17:00
Subj: Re: Various Warp 4 problems.

From: ysme@sympatico.ca

In <37FB90C2.1C8E8F93@io.com>, Mike DeSanto <desantom@io.com> writes:



>required Fix Pack 5.  I downloaded the CSF disk, the update disks, the
>Feature Install package and the latest Java Development Kit.
>
>I install the fix pack.  Next bootup, the system crashes.  It says
>something about ES1868$.  I boot with disks and find a line similar to
>DEVICE=D:\MMOS2\ESS1868DD.SYS /N:ES1868$.  I rem out that line and the
>next, which also uses the ES1868$.  OS/2 now boots, but my sound card
>does not work.  I try re-installing the card, no luck.


Their are several addresses listed in the readme info, that may not be used by 
any other
software, if NS 4.61 is to operate withour errors.  It may be time to read and 
print out 
that list, and use the RMView /DA > filename and start looking at both
printouts, to
get a hint of what happened.


--- WtrGate+ v0.93.p7 sn 165
 * Origin: Usenet: HARNESS the ABILITY dial up BBS 1-416-604-1221 (1:109/42)

+----------------------------------------------------------------------------+

+============================================================================+
