Next: Eckert IV and VI Up: Miscellaneous Projections Previous: Winkel Tripel Projection (–-Jr

## Robinson Projection (-–Jn -JN)

The Robinson projection, presented by Arthur H. Robinson in 1963, is a modified cylindrical projection that is neither conformal nor equal-area. Central meridian and all parallels are straight lines; other meridians are curved. It uses lookup tables rather than analytic expressions to make the world map ``look'' right5.2†. The scale is true along latitudes 38o. The projection was originally developed for use by Rand McNally and is currently used by the National Geographic Society. To use it you must enter

  The central meridian

  Scale along equator in inch/degree or 1:xxxxx (-Jn), or map width (-–JN)

Again centered on Greenwich, the example below was created by this command:

    pscoast -R-180/180/-90/90 -JN0/4.5i -Bg30/g15 -Dc -A10000 -G128 -P >! GMT_robinson.ps

Figure 5.29: World map using the Robinson projection