## NAME

          grdpaste - Paste together two .grd files along a common edge.

## SYNOPSIS

          grdpaste file_a.grd file_b.grd -Goutfile.grd [ -V ]

## DESCRIPTION

          grdpaste will combine file_a.grd and file_b.grd into outfile.grd by
          pasting them together along their common edge.  Files file_a.grd and
          file_b.grd must have the same dx, dy and have one edge in common.  If
          in doubt, check with grdinfo and use grdcut and/or grdsample if
          necessary to prepare the edge joint.

          file_a.grd
               One of two files to be pasted together.

          file_b.grd
               The other of two files to be pasted together.

          -Goutfile.grd
               The name for the combined output.

## OPTIONS

          -V   Selects verbose mode, which will send progress reports to stderr
               [Default runs "silently"].

## EXAMPLES

          Suppose file_a.grd is 150E - 180E and 0 - 30N, and file_b.grd is 150E
          - 180E, -30S - 0, then you can make outfile.grd which will be 150 -
          180 and -30S - 30N by:

          grdpaste file_a.grd file_b.grd -Goutfile.grd -V

## SEE ALSO

          gmt, grdcut, grdinfo, grdsample