Solution-Pac / E2
=================
CONTENTS

1) What you have to know
2) Information about pager/mail (Jericho)
   - Using MAPI-Mail driver
   - Session closure under Windows NT
   - Creating a new BIP driver

See also file <CD_DRIVE>:\README\README.TXT
              -----------------------------


1) What you have to know
========================

NT workstation : sending messages on UPS events
-----------------------------------------------
To allow the software to send messages, you must activate the 
NT message service on your station.

Windows systems : Messages for Novell environment
--------------------------------------------------
With some specifics operating system configurations, when our 
module named Jericho is starting, it could send the two 
following messages :
"IPX Not installed" and "Unable to start SPX" in two windows 
titled "Interface NetWare-Windows for Jericho".
If you want to be connected with a NetWare server, you have to 
check if the client for NetWare is correctly installed.
If you don't need to be connected to NetWare, it is possible to
suppress the two messages, modifing file 
UPSMAN\MMI\JERICHO\Jericho.ini
To do so, you have to disable the "Deport_Netware= ... " 
control key in section "[Modules] 
(adding comment character ";" at the beginning of the line)
NOTA :
The messages refered above will not disturb our software, 
except to communicate with a NetWare server.

CAUTION : Pager/Email functionality is not usable with PSP 
for NetWare. See MGE UPS Systems' Web site to get an update.

2) Information about pager/mail (Jericho)
=========================================
Using MAPI-Mail driver
----------------------

The MAPI-Mail driver of JERICHO uses the messaging interface 
of Windows 95/NT (MAPI). It can function only if the MICROSOFT 
EXCHANGE module is installed and correctly configured.
To open and configure Microsoft Exchange, double-click on the
Microsoft Exchange icon on the desktop.

Under Windows NT, when JERICHO is automatically launched, it 
functions as a service and is not attached to a user context. 
It has not therefore access to user profiles created by 
Microsoft Exchange.

To use the MAPI-Mail driver under Windows NT, it is necessary 
to launch JERICHO from the desktop (from the "Start" menu or 
by adding it to the "Startup" group).

The syntax to use to define the address of the receiver when 
dispatching a message through the MAPI-Mail driver depends on 
the messaging service selected. For the basic services 
installed under Windows 95 and Windows NT, this syntax is the 
following:

-> Internet Mail

	Use the e-mail address of the receiver

-> Microsoft Mail : 
	
	Use the syntaxe : NETWORK/POSTOFFICE/MAILBOX
	with
	NETWORK	     = network name (generally "Windows")
	POSTOFFICE   = MS-Mail server
	MAILBOX	     = mailbox of the receiver

To know parameters to use, open the address book of Microsoft 
Exchange ("Tools" menu) and double-click on the name of the 
desired receiver.

Session closure under Windows NT
--------------------------------

When JERICHO is automatically launched at Windows start, it is
running as a service. For reasons of to long closure time at 
Windows shutdown, JERICHO must anticipate its closure on 
receipt of log off message.
For this reason, JERICHO is stopped when the user logs off the
system.


Creating a new BIP driver
-------------------------

The "Bip" driver can be setup to call all type bips : bip 
service integrated to the enterprise pabx, person research 
system, public bip paging service.

When the bip driver is setup for use of a specific bip service,
it can be duplicated then renamed to make a new driver (as 
Tatoo).

To do it :

a) Setup the "Bip" driver with appropriate values and modify 
its name (for example : Bip -> Bip-New)

b) In the file "BIP.INI", at the "[Drivers]" entry, copy the 
first line ("0=Bip-New" in the example) and add it at the end 
of the entry with the number following the last defined 
driver. Then rename the first driver in the file.

	[Drivers]	---->		[Drivers]

	0=Bip-New			0=Bip
	1=Tatoo				1=Tatou
					2=Bip-New

c) In the file "PAGER.INI", at the "[Drivers]" entry, add a 
line to identify the new driver :

	[Drivers]
	Bip=100,Bip.DLL,0,1
	Tatoo=101,Bip.DLL,1,1

--->	[Drivers]
	Bip=100,Bip.DLL,0,1
	Tatoo=101,Bip.DLL,1,1
	Bip-New=102,Bip.DLL,2,1
