;------------------------------------------------------------------------------
; Copyright (c) 1993-1995 Microsoft Corporation
;
; v. 1.0 - Aug 05, 1996
; v. 1.1 - Apr 18, 1997 - compressed driver files
;
;------------------------------------------------------------------------------

[version]
signature="$CHICAGO$"
Class=hdc
Provider=%TBCH%

;Class Install
[ClassInstall]
AddReg=HDC_Class

[HDC_Class]
HKR,,,,%HDCClassName%
HKR,,Icon,,-9

[Manufacturer]
%Pinnacle-IDE%=PIN_IDE

[PIN_IDE]
%*PINIDE_250.DeviceDesc%   = PINIDE_250, *PNP0600        ;Generic_ESDI_Hard_Disk_Controller
%*PINIDE_260.DeviceDesc%   = PINIDE_260, *PNP0600        ;Generic_ESDI_Hard_Disk_Controller
%*PINIDE_270.DeviceDesc%   = PINIDE_270, *PNP0600        ;Generic_ESDI_Hard_Disk_Controller

[*pnp0600.det]          ;ESDI Controller
LogConfig=esdilc1
AddReg = HDC_HW_REG

; ------------------------------------------------------------------------

[PINIDE_250]
LogConfig=esdilc1
AddReg = ESDI_AddReg
CopyFiles=PINIDE.CopyList
UpdateCfgSys=PINIDE_250.UpdateCfgSys

[PINIDE_250.UpdateCfgSys]
DevDelete=pinide.sys
DevAddDev=pinide.sys,device,01, "/P:170 /I:15 /C:250"

; ------------------------------------------------------------------------

[PINIDE_260]
LogConfig=esdilc1
AddReg = ESDI_AddReg
CopyFiles=PINIDE.CopyList
UpdateCfgSys=PINIDE_260.UpdateCfgSys

[PINIDE_260.UpdateCfgSys]
DevDelete=pinide.sys
DevAddDev=pinide.sys,device,1, "/P:170 /I:15 /C:260"

; ------------------------------------------------------------------------

[PINIDE_270]
LogConfig=esdilc1
AddReg = ESDI_AddReg
CopyFiles=PINIDE.CopyList
UpdateCfgSys=PINIDE_270.UpdateCfgSys

[PINIDE_270.UpdateCfgSys]
DevDelete=pinide.sys
DevAddDev=pinide.sys,device,1, "/P:170 /I:15 /C:270"

; ------------------------------------------------------------------------

[PINIDE.CopyList]
pinide.sys,pinide.sy_,
tb-ide.sys,tb-ide.sy_,

[ESDI_AddReg]
HKR,,DriverDesc,,"ESDI Port Driver"
HKR,,DevLoader,,*IOS
HKR,,PortDriver,,ESDI_506.pdr

[HDC_HW_REG]
HKR,,NoSetupUI,,1


[esdilc1]
ConfigPriority=HARDWIRED
IOConfig=170-177(3ff::)
IOConfig=376-376(3ff::)
IRQConfig=S:15

; [esdilc2]
; ConfigPriority=HARDWIRED
; IOConfig=1f0-1f7(3ff::)
; IOConfig=3f6-3f6(3ff::)
; IRQConfig=S:14


[DestinationDirs]
DefaultDestDir = 10  

[SourceDisksNames]
1="Multisound Pinnacle Windows 95 Drivers",, 0001

[SourceDisksFiles]
pinide.sys=1
tb-ide.sys=1

[Strings]
HDCClassName = "Hard disk controllers"
TBCH = "Turtle Beach Systems"
Pinnacle-IDE= "Turtle Beach Systems"
*PINIDE_250.DeviceDesc = "Pinnacle IDE Controller (Control Port 250)"
*PINIDE_260.DeviceDesc = "Pinnacle IDE Controller (Control Port 260)"
*PINIDE_270.DeviceDesc = "Pinnacle IDE Controller (Control Port 270)"
